Router 0  
enable

configure terminal

hostname Router0

banner motd #Router0 - Khánh Hòa#

enable secret 123456

line console 0

password cisco

login

interface fa0/0

ip address 192.168.1.1 255.255.255.0

no shutdown

interface se2/0

ip address 10.0.0.1 255.255.255.252

clock rate 64000

no shutdown

router rip

version 2

no auto-summary

network 192.168.1.0

network 10.0.0.0

ROUTER1

enable

configure terminal

hostname Router1

banner motd #Router1 - Trung tâm#

enable secret 654321

line console 0

password cisco

login

interface fa0/0

ip address 192.168.2.1 255.255.255.0

no shutdown

interface se2/0

ip address 10.0.0.2 255.255.255.252

no shutdown

interface se3/0

ip address 10.0.0.5 255.255.255.252

clock rate 64000

no shutdown

router rip

version 2

no auto-summary

network 192.168.2.0

network 10.0.0.0

ROUTER 2

enable

configure terminal

hostname Router2

banner motd #Router2 - Dữ liệu#

enable secret 789123

line console 0

password cisco

login

interface fa0/0

ip address 192.168.3.1 255.255.255.0

no shutdown

interface se3/0

ip address 10.0.0.6 255.255.255.252

no shutdown

router rip

version 2

no auto-summary

network 192.168.3.0

network 10.0.0.0